# Release Notes

# Issues and notes for v1.9.38 2013.11.15

Known issues in version 1.9.38:

- "Mixed Format Frames on a CAN Network" (GMLAN) is implemented from the J2534-2 spec, but only for CAN_MIXED_MODE=1.
- The on-board clock cannot be set from web

# Release notes for v1.9.38 2013.11.15

The following fixes have been made in version 1.9.38:

- ISO9141: Fixed 5 baud init W1 delay, it was short by 18 ms.
- ISO9141: improved 5 baud init logging to show Key bytes received.
- J1708: limit baud rate to 19200 max.

# Release notes for v1.9.36 2013.02.14

The following fixes have been made in version 1.9.36:

- J1850 VPW, improved low speed reception issue on 2001 vehicles.
- Fixed J1708 time between messages after a collision.
- Added support for Clamp state (read V J1962 pin 1).

# Release notes for v1.9.34 2012.08.30

The following fixes have been made in version 1.9.34:

- J1850 VPW, improved sampling in high speed mode.
- Added support for J1850xxx_PS, ISO9141_PS and ISO14230_PS protocols.
- Fixed USB to Close the device when the USB cable is pulled.
- PassThruOpen pName accepts serial number only to open a specific device.

# Release notes for v1.9.32 2012.04.30

The following fixes have been made in version 1.9.32:

- CAN_PS, ISO15765_PS: Connect on pins 6,14 and 3,11 work simultaneously.
- ISO9141 and ISO14230: If Data bits set to 7, test check sum with 7 bits.
- ISO14230: Fixed the minimum P3 timeout for Fast Init.
- ISO9141: W5 in no longer supported per the J2534-1 spec.
- ISO14230: W0 is no longer supported per the J2534-1 spec.
- ISO9141 and ISO14230: reset W0 or W5 timer if byte(s) received.
- SW ISO15765: SW_HV_RX is now set when a high voltage message is received.
- ISO15765: 64 Flow Control Filters are now supported in -2 mode.

# Release notes for v1.9.30 2011.05.04

The following fixes have been made in version 1.9.30:

- ISO15765: Added support for N_xx timing parameters.

# Release notes for v1.9.28 2011.02.07

The following fixes have been made in version 1.9.28:

- PassThruRead/Write Msgs, NumMsgs set to zero on all errors.
- ISO15765: PassThruWriteMsgs with a timeout returns an error if a write message failed to transmit.
- ISO15765: Flow control filters distinguish between 11 bit and 29 bit settings.
- ISO15765: No longer waits stmin after receiving a flow control message.
- J2534-2: Discovery Mechanism returns correct error number for non-supported protocols.
- USB port scanned before Ethernet port so USB devices show up on top of Ethernet devices in the selection box.

# Release notes for v1.9.26 2010.08.15

The following fixes have been made in version 1.9.26:

- ISO15765 on _PS channel in Mixed Mode now allows PASS filters.
- Short to Ground allowed on Pin 15 when ISO9141 is connected.
- J2534-2: Discovery Mechanism no longer report Protocol Info for non-supported protocols.
- J2534-2: Fixed Single Wire CAN indications for speed change.

# Release notes for v1.9.24 2010.06.23

The following fixes have been made in version 1.9.24:

- Added support for Marvell 8385 PCMCIA cards.
- J2534-2: for _PS protocols PassThruIoctl SET_CONFIG J1962_PINS is required to connect.
- ISO15765: periodic no longer stops after receiving a segmented message.
- J1850PWM: minimum filter size is now 1 byte (was 3 bytes).
- Removed J2534 0202 DLL from the firmware package.
- ISO15765: Timeout values changed to match the ISO15765 specification.
- ISO14230: Fast Init, wait at least 50ms (ignore P3_MIN less than 50ms).
- ISO9141: Short to ground on pin 15 not allowed when L line in use.

# Release notes for v1.9.22 2009.12.10

The following fixes have been made in version 1.9.22:

- ISO15765 N_As timeout extended.
- Added J2534-2 XXX_SIMULTANEOUS support.

# Release notes for v1.9.20 2009.10.06

The following fixes have been made in version 1.9.20:

- CAN and ISO15765 baud rate calculation improved to hit more rates (667k)
- ISO15765 Mixed mode filter message validation improved
- ISO15765 restarts RX if Single Frame or First Frame received during RX.
- ISO14230 Fast init, L line asserted during break.
- ISO9141 5 baud init W1 time includes early check time of 70ms.
- ISO15765 Mixed mode no longer deletes Flow control filters.

# Release notes for v1.9.18 2009.03.04

The following fixes have been made in version 1.9.18:

- Fixed VPP control issue when switching SCI protocols after using SCI_TX_VOLTAGE.
- Changed ISO15765 interaction with Periodics to accomidate a Ford issue.
- Added J2534-2 Discovery Mechanism.
- Fixed ISO15765 STmin timer to meet spec. Time between, not start to start.
- Fixed debug log writing to support legacy directory enable.
- Fixed ISO9141 CS error on 24 byte boundaries.
- Improved Multi-thread error detection.

# Release notes for v1.9.16 2008.12.03

The following fixes have been made in version 1.9.16:

- Analog Protocol ID now matches J2534-2 (supports old value too, for now).
- J1708 now matches J2534-2 spec (priority in TxFlags).
- USB now works after closing an Ethernet connection.
- ISO14230 Fast Init now handles NULL parameters correctly.
- CLEAR_RX_BUFFER now gets all messages from driver before clear.
- ISO9141, ISO14230, delay P3_MIN after a break is received.
- Improved debug log name and saves to Logs directory.
- Fixed CLEAR_MSG_FILTERS to not report errors in debug log.
- Added cron and crontab to busy box.
- Added timestamp to Error returns in debug log.
- Installer no longer installs 0202 dll, no longer sets registry for 0202.
- Fixed default calculation of IP address for wireless configuration.